# Pi Servers -- Roadmap

## Alarm Configuration

Replace the current `randint(30, 60)` test loop in `contents_server.py` with real schedule-driven alarms.

### Config schema

File: `pi/alarm_config.json`

```json
{
  "alarm_time": "0700",
  "alarm_days": ["Mon", "Tue", "Wed", "Thu", "Fri"],
  "alarm_dates": ["07/20", "10/21"],
  "alarm_audio": "assets/alarm/alarm_test.wav",
  "alarm_image": "assets/img/on_alarm.png"
}
```

### Field definitions

| Field | Type | Description |
|-------|------|-------------|
| `alarm_time` | `string` | 4-digit HHMM (24-hour). Triggers on the 0th second of the minute, or as soon as Python detects it. |
| `alarm_days` | `string[]` | (Optional) 3-letter day abbreviations: `Mon`, `Tue`, `Wed`, `Thu`, `Fri`, `Sat`, `Sun`. Alarm only fires on listed days. If not supplied, alarms every day. |
| `alarm_dates` | `string[]` | (Optional) Strings of `MM/DD` format. If both `alarm_days` and `alarm_dates` are set, only `alarm_days` is effective. |
| `alarm_audio` | `string` | (Optional) Path to WAV file. Relative paths resolve from `pi/`. If not supplied, defaults to `assets/alarm/alarm_test.wav`. |
| `alarm_image` | `string` | (Optional) Path to status PNG shown during alarm. Relative paths resolve from `pi/`. If not supplied, defaults to `assets/img/on_alarm.png`. |

### Behavior

- On startup, load and validate `alarm_config.json`
- Each tick (~5s), check if current local time matches `alarm_time` and today's day name is in `alarm_days`, or if today's date is in `alarm_dates`.
- Fire alarm once per matched minute (debounce so it doesn't re-trigger within the same minute)
- After alarm completes, return to idle image and resume schedule checking

## Docker Compose

Containerize the pi servers for easier deployment.

### Options

1. **Single service** -- `run_all.py` as the entrypoint, both servers in one container
2. **Split services** -- separate containers for `stats_server.py` and `contents_server.py`

Single service is simpler. Split services allow independent scaling and restarts.

### Configuration

- Volume mount `assets/` and `alarm_config.json` so they're editable without rebuilding
- Expose ports 8765 and 8766
- Network mode `host` or a bridge with known IPs for ESP32 discovery
- Restart policy: `unless-stopped`

## Repository Extraction

The `pi/` directory will become its own git repository.

### Steps

1. Extract `pi/` into a standalone repo with its own `README.md`, `requirements.txt`, and CI
2. Add it back to this project as a git submodule
3. The interface contract between the two repos is the WebSocket protocol -- JSON schemas and binary frame formats documented in `docs/ALARM_PROTOCOL.md`

### Benefits

- Independent versioning and release cycle
- Pi-side contributors don't need the ESP-IDF toolchain
- CI can test the Python servers in isolation
- Cleaner separation of concerns between embedded firmware and host services
